#### *2019 new products*

#### rimfire Rifle & Handgun

Clean-22

The future of rimfire is here. New CCI® Clean-22™ uses an exclusive polymer bullet coating to greatly reduce copper and lead fouling in the barrel—without leaving a residue. It also cuts lead buildup in suppressors 60 to 80 percent. Both the Sub-Sonic and High Velocity loads feature a 40-grain round nose lead bullet with geometry that’s been optimized for accuracy. With dependable CCI priming and consistent propellant, Clean-22 provides flawless cycling through semi-automatics and all 22 LR firearms.

Features & Benefits

* Polymer bullet coating greatly reduces lead fouling in the barrel without leaving residue
* Cuts lead buildup in suppressors 60 to 80 percent
* 40-grain lead round nose bullets—red for High Velocity, blue for Sub-Sonic
* Optimized bullet geometry for improved accuracy
* Reliable function in semi-automatic firearms
* Great option both casual and competitive shooters

Part No. Description UPC MSRP

934CC Sub-Sonic 22 LR 40-grain blue poly-coated LRN, 1070 fps, 100-count 6-04544-65031-0 $9.95

944CC High Velocity 22 LR 40-grain red poly-coated LRN, 1235 fps, 100-count 6-04544-65032-7 $9.95

