Reloder TS 11

Craft more accurate, consistent varmint and benchrest loads with the new Reloder® TS 11 from Alliant Powder®. The propellant’s sophisticated TZ® technology manipulates the response of the material and resists the natural tendency to generate more pressure at higher temperatures and less pressure at lower temperatures. As a result, it delivers extremely consistent velocities across the temperature spectrum. Reloder TS 11 contains no dinitrotoluene or phthalate-based deterrents, so it is REACH-compliant. The patented decoppering agent helps keep copper from building up in the bore, so you shoot more and clean less.

Features & Benefits

* Extremely temperature stable
* Formulation is ideal for use in varmint loads
* Excellent burn speed for short-range benchrest applications
* Contains de-coppering agent
* Excellent lot-to-lot consistency
* REACH-compliant

Part No. Description MSRP

151004 Reloder TS 11 1-pound canister $44.99

151005 Reloder TS 11 8-pound canister $335.99

Graphical user interface

Description automatically generated with low confidence

TZ is a registered trademark of EURENCO Bofors AB