**110 WOLVERINE**

**SAVAGE ARMS 2018**

**110 WOLVERINE**

Chambered for the straight-walled 450 Bushmaster cartridge, the Savage 110 Wolverine offers both precision and power for deer, bears and hogs. Its AccuFit™ system lets you easily tailor the length-of- pull and comb height for a perfect fit, while the user-adjustable AccuTrigger™ offers a crisp, clean pull. Together with the AccuStock™, which secures the action three-dimensionally along its entire length, the 110 Wolverine provides the fit and function of a custom rifle—right out of the box. It features a Magpul AICS magazine, as well as an 18-inch carbon steel heavy barrel with a ported muzzle brake and 11/16- 24 threading. A one-piece 0 MOA rail mounted on the receiver makes it easy to set up the rifle to your unique needs.

# FEATURES:

## AccuFit system lets shooters quickly adjust comb height and length-of-pull

* User-adjustable AccuTrigger
* AccuStock rail system secures the action three-dimensionally along its entire length
* Tough synthetic stock
* 18-inch carbon steel heavy barrel
* Ported muzzle brake and 11/16-24 threading
* 5-round Magpul AICS magazine
* One-piece 0 MOA rail mounted on the receiver
* Soft grip fore-end and pistol grip surfaces
* New Model 110 design and ergonomics



|  |  |
| --- | --- |
| MANUFACTURER | SAVAGE ARMS |
| IMPORTER | N/A |
| ACTION TYPE | BOLT |
| FINISH | BLACK MATTE BARREL |
| SIGHTS | NONE |
| TRIGGER PULL WEIGHT | 2.5 LBS. – 6 LBS. |
| STOCK | GRAY SYNTHETIC STOCK |
| ACCESSORIES | COMB HEIGHT INSERTS AND LENGTH OF PULL INSERTS |
| OVERALL LENGTH | 37.5”- 38.5” |
| WEIGHT | 7.9 LBS. |
| DROP AT COMB | 1.10”-0.30” |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PART NO.** | **CALIBER** | **TWIST RATE** | **BARREL LENGTH** | **CAPACITY** | **UPC** | **MSRP** |
| 57140 | 450 BUSHMASTER | 1 IN 24” | 18” | 4+1 | 0-11356-57140-3 | $899 |

savagearms.com Copyright © 2017 Vista Outdoor